To: Cooling
From: Power
Subject: Bulkheads

Bulkhead doors should remain closed (green) at all times, unless otherwise directed by senior staff, to prevent unnecessary backflow.

OBO, Prof Ziglitz.

Production Dept.