To: Cooling
From: Power
Subject: Bulkheads

Water channels should be checked for blockages, else bulkhead doors should remain closed at all times unless otherwise directed by senior staff to prevent unnecessary backflow and flooding of facility with pre-processed water for heavy production.

OBO, Prof Ziglitz.

Production Dept.